IZAR III ZLI3.L4.1500.XY
Type: suspension lamp. Lampshade: acrylic glass, front white (.92) or black (.93). Metal parts: white painted steel plate. Pendant: steel wire suspension with a transparent cable.
Voltage: 230V
IK code: IK06
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 26,5 W
Color temperature: 4000 K
Module luminous flux: 3815 lm
Luminaire luminous flux: 3504 lm
A: 1500 mm
B: 80 mm
C: 2000 mm
D: 40 mm
Dali 2: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Track system: Available on inquiry
Sádrokarton: Available on inquiry
Weight: 4200 g