Description

POLARIS ZKS ZKS.L4.400.XY
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9003 (.31), RAL 9005 (.61), RAL chrom (.77), chrome (.80) or brass (.84). Pendant: white or black self-carrying conductor reinforced with a steel wire.
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 18,3 W
Color temperature: 4000 K
Module luminous flux: 2892 lm
Luminaire luminous flux: 2574 lm
A: 400 mm
C: 2000 mm
Dali 2: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Sádrokarton: Available on inquiry
CRI > 90: Available on inquiry
Weight: 4900 g

LUCIS, s. r. o., Heršpická 814/5a, 639 00  Brno, Tel.: +420 543 248 881, E-mail: info@lucis.eu