Description

ALFA ZK1.L1.200.XY
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9003 (.60) or RAL 9005 (.61). Pendant: white or black cable.
Voltage: 230V
IK code: IK01
CRI: >80
LED life: L80/F10 50000 hours
Watt: 8 W
Color temperature: 3000 K
Module luminous flux: 656 lm
Luminaire luminous flux: 558 lm
A: 200 mm
B: 2000 mm
Track system: Available on inquiry
Phase-cut dimming: Available on inquiry
Weight: 1400 g

LUCIS, s. r. o., Heršpická 814/5a, 639 00  Brno, Tel.: +420 543 248 881, E-mail: info@lucis.eu