Description

IZAR C ZL1.IC.K1.330.91Y
Type: suspension lamp. Lampshade: acrylic glass. Light body: white painted steel plate. Pendant: steel wire suspension with a transparent cable.
Voltage: 230V
IK code: IK06
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 26 W
Color temperature: 3000 K
Module luminous flux: 3329 lm
Luminaire luminous flux: 2691 lm
A: 330 mm
B: 330 mm
C: 2000 mm
D: 330 mm
Dali 2: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Track system: Available on inquiry
Sádrokarton: Available on inquiry
Weight: 3700 g

LUCIS, s. r. o., Heršpická 814/5a, 639 00  Brno, Tel.: +420 543 248 881, E-mail: info@lucis.eu