Description

IZAR C IC.K3.440.X
Type: ceiling and wall lamp. Lampshade: acrylic glass, sides white (.91) or black (.93). Light body: white painted steel plate.
Voltage: 230V
IK code: IK06
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 26,9 W
Color temperature: 3000 K
Module luminous flux: 3329 lm
Luminaire luminous flux: 2766 lm
A: 440 mm
Dali 2: Available
Corridor function: Available on inquiry
Motion sensor: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Track system: Available
Weight: 7800 g

LUCIS, s. r. o., Heršpická 813/5, 639 00  Brno, Tel.: +420 543 248 881, E-mail: info@lucis.eu