Description

IZAR C IC.L2.250.XY
Type: ceiling and wall lamp. Lampshade: acrylic glass, sides white (.91) or black (.93). Light body: white painted steel plate.
Voltage: 230V
IK code: IK06
Ballast: Driver
CRI: >80
LED life: L80/F10 50000 hours
Watt: 10,5 W
Color temperature: 4000 K
Module luminous flux: 1600 lm
Luminaire luminous flux: 1290 lm
A: 250 mm
Dali 1: Available
Dali 2: Available
Corridor function: Available on inquiry
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Weight: 3300 g

LUCIS, s. r. o., Heršpická 813/5, 639 00  Brno, Tel.: +420 543 248 881, E-mail: info@lucis.eu