Description

ZERO ZL3.412.Z500 EVG
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9006 structured. Pendant: steel wire suspension with a transparent cable.
Voltage: 230V
IK code: IK01
ballast: EVG
Socket: 2GX13
Lamps: 1×22W+1×40W
A: 500 mm
B: 90 mm
C: 2000 mm
Weight: 8200 g

LUCIS, s. r. o., Heršpická 813/5, 639 00  Brno, Tel.: +420 543 248 881, E-mail: info@lucis.eu