Description

DAPHNE S34.L1.D450.Y
Type: ceiling and wall lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Light body: white painted steel plate.
Voltage: 230V
IK code: IK01
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 37,1 W
Color temperature: 3000 K
Module luminous flux: 4824 lm
Luminaire luminous flux: 3570 lm
A: 450 mm
B: 180 mm
C: 20 mm
D: 340 mm
Dali 2: Available
Motion sensor: Available on inquiry
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Weight: 4500 g

LUCIS, s. r. o., Heršpická 814/5a, 639 00  Brno, Tel.: +420 543 248 881, E-mail: info@lucis.eu