IZAR C ZL1.IC.L2.330.91Y
Type: suspension lamp. Lampshade: acrylic glass. Metal parts: white painted steel plate. Pendant: steel wire suspension with a transparent cable.
Voltage: 230V
IK code: IK06
Ballast: Driver
CRI: >80
LED life: L80/F10 50000 hours
Watt: 11,3 W
Color temperature: 4000 K
Module luminous flux: 1951 lm
Luminaire luminous flux: 1580 lm
A: 330 mm
B: 330 mm
C: 2000 mm
D: 330 mm
Dali 1: Available
Dali 2: Available
Corridor function: Available on inquiry
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Track system: Available on inquiry
Weight: 5200 g