SEMILUNA ZT.11.S200.X
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9003 (.60), RAL 9005 (.61), RAL Bronze (.73) or RAL Chrom (.77). Pendant: rod.
Voltage: 230V
IK code: IK01
Socket: E27
Lamps: 1x60(46)W
A: 200 mm
C: 1000 mm
Track system: Available on inquiry
Weight: 2100 g