IZAR C IC.K2.330.X
Type: ceiling and wall lamp. Lampshade: acrylic glass, sides white (.91) or black (.93). Light body: white painted steel plate.
Voltage: 230V
IK code: IK06
Ballast: Driver
CRI:  >90
LED life: L80/F10 50000 hours
Watt: 26 W
Color temperature: 4000 K
Module luminous flux: 3488 lm
Luminaire luminous flux: 2820 lm
A: 330 mm
Dali 2: Available
Corridor function: Available on inquiry
Motion sensor: Available
Emergency module: Available on inquiry
Bluetooth control: Available on inquiry
Track system: Available
Weight: 3300 g