ZERO ZL3.411.Z415 EVG
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9006 structured. Pendant: steel wire suspension with a transparent cable.
Voltage: 230V
IK code: IK01
ballast: EVG
Socket: 2GX13
Lamps: 1×55W
A: 415 mm
B: 80 mm
C: 2000 mm
Weight: 5300 g