Description

POLARIS ZK ZK.11.500.X
Type: suspension lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Metal parts: painted steel plate RAL 9003 (.31), RAL 9005 (.61), RAL chrom (.77), chrome (.80), stainless steel (.83) or brass (.84). Pendant: white or black self-carrying conductor reinforced with a steel wire.
Voltage: 230V
IK code: IK01
Socket: E27
Lamps: 1×200(140)W
A: 500 mm
C: 2000 mm
Weight: 6700 g

LUCIS, s. r. o., Heršpická 814/5a, 639 00  Brno, Tel.: +420 543 248 881, E-mail: info@lucis.eu