Description

LEDA S29.12.JS33.Y
Type: ceiling and wall lamp, type S37.xxx only as the ceiling lamp. Lampshade: white, hand-blown, three-layered glass, satin opal matt. Light body: white painted steel plate.
Voltage: 230V
IK code: IK01
Socket: E27
Lamps: 2×75(57)W
A: 330 mm
B: 290 mm
C: 200 mm
Motion sensor: Available on inquiry
Weight: 2700 g

LUCIS, s. r. o., Heršpická 814/5a, 639 00  Brno, Tel.: +420 543 248 881, E-mail: info@lucis.eu